HKG01_RE1> show route 172.16.128.2 

inet.0: 692051 destinations, 3523520 routes (691742 active, 61 holddown, 1019 hidden)
+ = Active Route, - = Last Active, * = Both

172.16.128.2/32    *[LDP/9] 00:53:16, metric 6
                    > to 192.168.146.37 via ae8.1, Push 302432
                      to 192.168.147.33 via xe-1/3/2.1, Push 318768
                    [OSPF/10] 00:54:56, metric 6
                    > to 192.168.146.37 via ae8.1
                      to 192.168.147.33 via xe-1/3/2.1

HKG01_RE1> show route 192.168.144.6 

inet.0: 691822 destinations, 3523772 routes (691559 active, 15 holddown, 1014 hidden)
+ = Active Route, - = Last Active, * = Both

192.168.144.6/32   *[LDP/9] 01:19:18, metric 6
                    > to 192.168.144.33 via xe-2/1/3.0, Push 410112
                    [OSPF/10] 2d 01:49:10, metric 6
                    > to 192.168.144.33 via xe-2/1/3.0

HKG01_RE1> show ospf neighbor 
Address          Interface              State     ID               Pri  Dead
192.168.146.37   ae8.1                  Full      192.168.146.6    128    39
192.168.147.33   xe-1/3/2.1             Full      192.168.147.2    128    32
192.168.144.33   xe-2/1/3.0             Full      192.168.144.2    128    34

HKG01_RE1> show configuration protocols ospf       
traffic-engineering;
area 0.0.0.0 {
    interface lo0.0;
    interface ae8.1 {
        interface-type p2p;
        link-protection;
        bfd-liveness-detection {
            minimum-interval 100;
        }
    }
    interface xe-1/3/2.1 {
        interface-type p2p;
        link-protection;
        metric 5;
        bfd-liveness-detection {
            minimum-interval 100;
        }
    }
   interface xe-2/1/3.0 {
        interface-type p2p;
        metric 5;
        bfd-liveness-detection {
            minimum-interval 100;
        }
    }

HKG01_RE1> show configuration routing-options
backup-selection {
    destination 0.0.0.0/0 {
        interface all {
            evaluation-order metric;
        }
    }
}
========================================================================

HKG02_RE1> show route 172.16.128.2 

inet.0: 694834 destinations, 4320686 routes (691725 active, 13 holddown, 777315 hidden)
+ = Active Route, - = Last Active, * = Both

172.16.128.2/32    *[LDP/9] 00:55:03, metric 5
                    > to 172.16.128.41 via xe-1/2/2.0
                    [OSPF/10] 00:56:42, metric 5
                    > to 172.16.128.41 via xe-1/2/2.0

HKG02_RE1> show route 192.168.144.6 

inet.0: 694639 destinations, 4319477 routes (691490 active, 14 holddown, 777159 hidden)
+ = Active Route, - = Last Active, * = Both

192.168.144.6/32   *[LDP/9] 01:21:28, metric 7
                    > to 192.168.146.38 via ae8.1, Push 300864
                      to 182.54.128.41 via xe-1/2/2.0, Push 305344
                    [OSPF/10] 01:23:11, metric 7
                    > to 192.168.146.38 via ae8.1

HKG02_KATRINA_RE1> show ospf neighbor       
Address          Interface              State     ID               Pri  Dead
192.168.146.38   ae8.1                  Full      192.168.146.2    128    32
1172.16.128.41    xe-1/2/2.0             Full      172.16.128.2     128    38

HKG02_RE1> show configuration protocols ospf                 
traffic-engineering;
export EXPORT-TO-OSPF;
area 0.0.0.0 {
    interface lo0.0;
    interface ae8.1 {
        interface-type p2p;
        link-protection;
        bfd-liveness-detection {
            minimum-interval 100;
        }
    }
        interface xe-1/2/2.0 {
        interface-type p2p;
        link-protection;
        metric 5;
        bfd-liveness-detection {
            minimum-interval 100;
        }
    }
    }

HKG02_RE1> show configuration routing-options
backup-selection {
    destination 0.0.0.0/0 {
        interface all {
            inactive: evaluation-order metric;
        }
    }
}