**root@X49-D40-6> show version**

Hostname: X49-D40-6

Model: vSRX

Junos: 15.1X49-D40.6

JUNOS Software Release [15.1X49-D40.6]

**root@X49-D40-6> show chassis hardware**

Hardware inventory:

Item Version Part number Serial number Description

Chassis c69fde3c7817 VSRX

Midplane

System IO

Routing Engine VSRX RE

FPC 0 Virtual FPC

Power Supply 0

**root@X49-D40-6> show chassis fpc pic-status**

Slot 0 Present Virtual FPC

**root@X49-D40-6> show chassis fpc pic-status**

Slot 0 Present Virtual FPC

**root@X49-D40-6> show interfaces terse**

Interface Admin Link Proto Local Remote

dsc up up

em0 up up

em0.0 up up inet 128.0.0.1/2

em1 up up

em1.32768 up up inet 192.168.1.2/24

em2 up up

fxp0 up up

fxp0.0 up up inet 192.168.0.10/24

gre up up

ipip up up

irb up up

lo0 up up

lo0.16384 up up inet 127.0.0.1 --> 0/0

lo0.16385 up up inet 10.0.0.1 --> 0/0

10.0.0.16 --> 0/0

128.0.0.1 --> 0/0

128.0.0.4 --> 0/0

128.0.1.16 --> 0/0

lo0.32768 up up

lsi up up

mtun up up

pimd up up

pime up up

pp0 up up

ppd0 up up

ppe0 up up

st0 up up

tap up up

vlan up down

**root@X49-D40-6% ps aux | grep srxpfe**

root 1867 4.0 0.1 2088 1248 p0 S+ 11:18PM 0:00.02 grep srxpfe

**root@X49-D40-6% vty fpc0**

connect: Connection refused

protocol setup: Connection refused

Connection Failure: Connection refused